3D CAD models for version 2 of the Uzebox enclosure fitted with type 2 SNES connectors.

<img src="assets/uzebox-enclosure-v2.jpg" alt="Uzebox Enclosure V2" height="300"  /> <img src="assets/snes_conn_models.jpg" alt="SNES connectors type" height="300" />

<img src="assets/top-shell.png" alt="Top Shell" height="75"/><img src="assets/bottom-shell.png" alt="Shell" height="75"/><img src="assets/cover.png" alt="Cover" height="75"/><img src="assets/power-button.png" alt="Power Button" height="75"/><img src="assets/reset-button.png" alt="Reset Button" height="75"/><img src="assets/logo.png" alt="Logo" height="75"/><img src="assets/text.png" alt="Text" height="75"/>

### Notes
* Version 2.0 has a cutaway at the back of the top shell to allow the use of right-angled ISP sockets.
* Models provided in .3MF and Autodesk Fusion360 zipped project format. 
* Tips and tricks on 3D printing and modifications to the case can be found on the [Uzebox WIKI](https://uzebox.org/wiki/3D_printed_case).

### Compatible with the folowing Uzebox versions
* [Uzebox (All revisions)](https://github.com/Uzebox/uzebox/tree/MoveEagleAndCADtoGit/schematics/Uzebox/V5.0)
* Uzebox Omega


